

**Asbestos Management Plan template**

Asbestos will be removed when either building projects touch the affected area or it becomes hazardous. Any other areas with asbestos will be inspected annually by members of the congregation. Every five years they will be inspected by a qualified person. These inspections will be recorded.

If any damage to asbestos is found then this will either be made safe or removed by approved people and such actions recorded in the register.

* The area will be marked as a no go area until the problem is resolved.
* Properly painted to seal all asbestos. Any breaks of the seal will immediately be appropriately resealed or the asbestos removed.
* In either case the asbestos will be reinspected after the work is done

Asbestos affects people working on the site:

* Any builders working on the site will be formally shown the asbestos register.
* In the case of sale where the asbestos has not been removed, the purchaser will be informed of the presence of asbestos.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| A group of planes flying in formation  Description automatically generated with medium confidence**Date of Inspection** | **Person Inspecting** | **Issues Found** | **Action Needed/ Completed** | **Date when Work done** | **Date when successfully reinspected** | **Next Inspection** | **Next Five Year (external) Inspection** |
|  |  |  |  |  |  |  |  |
| *Hall* |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| *Manse* |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| *Church building* |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| *Other* |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |